|  |  |  |
| --- | --- | --- |
| Important | Semi-Important | Not-Important |
| TSCWT1 (Turbine Load MW) | MFWFT511*/521* (Trip-related parameter) (Downcomer L) | RRCNP10 (Power in Percentages) |
| RCSCT5 (Boron Concentration) | MRSFT512*/522/523* (SG Flow 1A) | RCSTT499B (Reference Temperature) |
| MRSPT514*/524/534/544*  (Pressure of SG1 Loop 1A) | MRSFT510*/520* (Total SG Flow) | RRCYT100 (Rod Position) |
| RCSLT501*/502* (SG Wide ring level) | RCSTT451A/452A (Pressurizer Spray Water A Temperature) | MGPWT11 (Generated Power) |
| RCSFT414  (Flow of Cold Leg of Loop 1 A) | RCSTT450B (Pressurizer Surge Line Temperature) | RCSPV455B*/455C* |
| RCSFT424  (Flow of Cold leg of Loop 1B) | HPCFT918  (Flow of discharge from Pump A) (It equalizes at about 50) | Column 24 |
| RCSLT470  (Pressurizer Relief Tank Level) |  | RCSLT517A*/527A* (Narrow Ring Level) |
| RCSPT405 (Wide Ring Channel 1 Pressure) |  | AFWFT2 (column 28) |
| RCSTT413A (Wide Ring Hot Leg SG1 Temperature) |  | AFWFT9 (column 29) |
| RCSTT413B  (Wide Ring Cold Leg 1A Temperature) |  | RCSFT434 |
| RCSTT423B (Wide Ring Cold Leg 1B Temperature) |  | RCSFT444 |
| RCSTT423C (Wide Ring Hot Leg SG1 Temperature) |  | RCSLT459  (Pressurizer Level) |
| RCSTT433B (Wide Ring Cold Leg 2A Temperature) |  | RCSPT403 |
| RCSTT443B (Wide Ring Cold Leg 2B Temperature) |  | RCSPT455A  (Equating to Containment Pressure) |
| RCSTT453A (Pressurizer Water Temperature) |  | RCSPT469A  (Pressurizer Relied Tank Pressure) |
| RCSTT1734 (??)  (Margin to Saturation RNA) |  | RCSTT400A (Average Temperature of Loop 1A) |
| CTMTT60 (73)  (Containment Temperature) |  | RCSTT420A |
| CTMPT1000A (72) (Containment Pressure) |  | RCSTT454 |
| RRCTP10 (10)  (Thermal Power) |  | RCSTT468A |
|  |  | RCSTC502 (Average Temperature of RCS) |
|  |  | RCSTT1735 (Margin to Saturation RNA) |
|  |  | CVCFT121 |
|  |  | CVCFT132A (58) |
|  |  | CVCFT145A (59) |
|  |  | CVCFT161B (60) |
|  |  | RHRFT988 (61) |
|  |  | HPCFT922 (63) |
|  |  | CSSFT5 (64) |
|  |  | CSSFT11 (65) |
|  |  | ASILT950 (66) |
|  |  | ASILT952 (67) |
|  |  | ASILT954 (68) |
|  |  | MGPWT1 (69) |
|  |  | ASILT956 (70) |
|  |  | CTMCT27 (71) |
|  |  | CPSRT591 (74) |
|  |  | MGPWT01 (75) |
|  |  | HPCPT947 (76) |